|  |  |  |
| --- | --- | --- |
|  | Your company nameWorkplace Safety AssessmentJob Hazard Analysis (JHA)  | Your logo here |
| Document Control #: | Stone-JHA-005 | Revision Date: | mm/dd/yyyy |
| Document Title: | Job Hazard Analysis (JHA) | Issue #: | 1.0 |
| Department: | Warehousing | Frequency: | Annually |
| Personal Protective Equipment Required: | Safety glasses, gloves, safety vest  | Completed by: | Name of Company Representative Here |
| Using a Nail Gun |
| Task Description | Hazard | Control |
| Splinter or blow out fragments from the material being nailed | Eye / skin | * Wear safety glasses
 |
| Puncture the back of the material | Product damage / Operator injury | * Set firing pressure at manufacturer’s recommendations
* Do not defeat safety devices
* Keep hands and feet clear at all times
 |
| Fire completely through the material | Strike workers behind the nailing surface / Product damage | * Set firing pressure at manufacturer’s recommendations
* Do not defeat safety devices
 |

Rationale or Comment:

* + Only use a sequential style nail gun, these do not allow bump firing. The nose has to be depressed before the trigger can be pulled.
	+ Keep finger off trigger when not driving nails.
	+ Avoid line of fire hazards in front of and behind material; position yourself (especially your free hand) out of the line of fire. Never point nail gun at anyone. Watch for coworkers behind the nailing surface.
	+ Disconnect/remove power source from gun to perform maintenance, move to another work area, or clear jams.
	+ Train on safe operating procedures, proper body placement and correct PPE use.

End of Document

**Disclaimer**

*This document is written as a general guideline. MIA+BSI and its Member companies have neither liability nor can they be responsible to any person or entity for any misunderstanding, misuses, or misapplication that would cause loss or damage of any kind, including loss of rights, material, or personal injury, or alleged to be caused directly or indirectly by the information contained in this document.*