|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
|  | Your company name  Workplace Safety Assessment  Job Hazard Analysis (JHA) | | | | Your logo here |
| Document Control #: | Stone-JHA-016 | | | Revision Date: | mm/dd/yyyy |
| Document Title: | Job Hazard Analysis (JHA) | | | Issue #: |  |
| Department: | (name) | | | Frequency: | (Annually, monthly, weekly) |
| Personal Protective Equipment Required: | Hardhat, safety glasses, respirator, gloves, safety vest | | | Completed by: | Name of Company Representative Here |
| Mixing Mortar | | | | | |
| Task Description | | Hazard | Control | | |
| Mixing mortar with mortar box or gas/electric mortar mixer | | Eye or extremity injury  Dust inhalation  Skin irritation | * Connect mixer to a Ground Fault Circuit Interrupter (GFCI) outlet * Do not use extension cords without a grounding wire * Lift properly using legs and keeping back straight * Confirm area is free of debris at all times * Empty bags low in mortar box to reduce dust * Keep room closed off with plastic at door * No other trades or workers are permitted in work space * Keep exposed skin clean at all times when using portland products * Always wash mortar off skin | | |

Rationale or Comment:

* + All employees will be fit tested and medically evaluated for respirator use by a Professionally Licensed Health Care Professional.

End of Document

**Disclaimer**

*This document is written as a general guideline. MIA+BSI and its Member companies have neither liability nor can they be responsible to any person or entity for any misunderstanding, misuses, or misapplication that would cause loss or damage of any kind, including loss of rights, material, or personal injury, or alleged to be caused directly or indirectly by the information contained in this document.*