|  |  |  |
| --- | --- | --- |
|  | Your company nameWorkplace Safety AssessmentJob Hazard Analysis (JHA)  | Your logo here |
| Document Control #: | Stone-JHA-017 | Revision Date: | mm/dd/yyyy |
| Document Title: | Job Hazard Analysis (JHA)  | Issue #: |  |
| Department: | (name) | Frequency: | (Annually, monthly, weekly) |
| Personal Protective Equipment Required: | Hardhat, safety glasses, face shield, dust mask, gloves, safety vest  | Completed by: | Name of Company Representative Here |
| Mixing Thinset or Grout with an Electric Drill |
| Task Description | Hazard | Control |
| Mixing thinset or grout with an electric drill | Eye InjuryDust InhalationSkin Irritation  | * Do not use extension cords without a grounding wire
* Keep exposed skin clean at all times when using portland products
* Immediately wash thinset or grout off skin
* Isolate mixing area from other trade to avoid dust exposure
 |

Rationale or Comment:

* + Connect drill to a Ground Fault Circuit Interrupter (GFCI) outlet

End of Document

**Disclaimer**

*This document is written as a general guideline. MIA+BSI and its Member companies have neither liability nor can they be responsible to any person or entity for any misunderstanding, misuses, or misapplication that would cause loss or damage of any kind, including loss of rights, material, or personal injury, or alleged to be caused directly or indirectly by the information contained in this document.*