|  |  |  |
| --- | --- | --- |
|  | Your company nameWorkplace Safety AssessmentJob Hazard Analysis (JHA)  | Your logo here |
| Document Control #: | Stone-JHA-028 | Revision Date: | mm/dd/yyyy |
| Document Title: | Job Hazard Analysis (JHA)  | Issue #: |  |
| Department: | Fabrication shop | Frequency: | (Annually, monthly, weekly) |
| Personal Protective Equipment Required: | Hardhat, steel toe shoes, safety glasses, gloves, safety vest, hearing protection as required.  | Completed by: | Name of Company Representative Here |
| Fabricator |
| Task Description | Hazard | Control |
| Prepares job, lifts stone to and from cart, uses hand saws, electric router, and hand grinders. Housekeeping.  | Ergonomic: strains and sprains from attempting to lift large loads | * Single employee restricted not to lift over 100 lbs.
* Ergonomic training conducted during safety meetings.
* Lift properly using legs, keeping back straight
* Complete back safety training
 |
|  | Noise: this area found to exceed 85 dB | * Hearing protection required, written conservation program, annual hearing tests given
 |
|  |  Slip, trip and fall | * Good housekeeping required
* Slip resistant boots required
* Turns lights on in work area
* ALWAYS Look where you are going – do not assume there is a clear path
 |
|  | Struck by  | * Employee walking with stone trained not to stand under or in front of moving load (fall shadow)
* Traffic areas cleared so stone cart has smooth operating surface
* Hard hats required during crane operation.
 |
|  | Mechanical failure | * Machine automatically shuts down if capacity exceeded
 |
|  | Mechanical vibration | * Employee trained to stretch and exercise hands and arms during breaks
 |
|  | Chemical (toxic, flammable) | * Review SDS for sealers and glue in use.
* No smoking
 |
|  | Electrical (loss of power) | * Machinery stops automatically and will not self-start
* Employees trained to power off machine prior to switching breaker back on
 |
|  | Temperature extreme  | * Complete Heat Stress /heat stroke training
 |

Rationale or Comment:

* + All employees must wear company-supplied steel toe shoes.
	+ Exercise caution at all times.

End of Document

**Disclaimer**

*This document is written as a general guideline. MIA+BSI and its Member companies have neither liability nor can they be responsible to any person or entity for any misunderstanding, misuses, or misapplication that would cause loss or damage of any kind, including loss of rights, material, or personal injury, or alleged to be caused directly or indirectly by the information contained in this document.*